DOOR TRIM PAD RATTLE (REPLACE/ INSPECT, CLIPS & SCREWS). Cadillac Concours 1994

For 1990-2009 cars

# DOOR TRIM PAD RATTLE (REPLACE/ INSPECT, CLIPS & SCREWS)

REVISION: 10/05/95

THIS BULLETIN IS BEING REVISED TO ADD THE 1994-95 MODEL YEARS AND TO UPDATE PARTS AND WARRANTY INFORMATION. **********************************************************************

#### SUBJECT: DOOR TRIM PAD RATTLES (DIAGNOSE/REPLACE CLIPS, INSPECT SCREWS, WRAP FOAM TAPE AROUND DOOR HOOK/BELT LINE CLIPS)

#### MODELS: 1992-95 CADILLAC ELDORADO, SEVILLE

PREVIOUS DIVISIONAL PUBLICATION NUMBERS WERE:

CADILLAC: T-92-127 GM OF CANADA: 93-10-111

#### CONDITION:

SOME OF THE ABOVE MODELS MAY EXHIBIT A RATTLING AND/OR LOOSENESS IN THE DOOR TRIM PAD AREA.

#### CAUSE:

THIS CONDITION MAY BE DUE TO THE FIT OF THE DOOR TRIM PAD TO THE DOOR INNER PANEL.

#### CORRECTION:

TO REPAIR THIS CONDITION, USE THE FOLLOWING PROCEDURE:

1. REMOVE DOOR TRIM PAD. REFER TO SECTION 10-6 OF THE SERVICE MANUAL.

#### IMPORTANT: THE ELDORADOS HAVE A HIDDEN SCREW IN THE UPPER REAR AREA OF THE CARPET INSERT AND THE SEVILLE REAR DOOR TRIM PADS MAY HAVE AN ADDITIONAL SCREW IN THE CARPET AREA.

2. IF THE SEVILLE DOOR TRIM PAD FITS LOOSE ALONG THE TOP EDGE AND THE CLIPS ARE BLACK, REPLACE WITH SILVER CLIPS.

3. INSPECT SPEAKER FOR MISSING, LOOSE, OR STRIPPED ATTACHING SCREW. REPAIR OR REPLACE AS NECESSARY.

4. CHECK DOOR PANEL FOR LOOSE STOCK.

5. WRAP FOAM TAPE FROM KENT INDUSTRIES, P/N 40100 (5/8" X 1/8" ADHESIVE-BACKED SHIM STOCK), OR EQUIVALENT AROUND EACH DOOR HOOK AND ON ELDORADO BELT LINE CLIPS. (SEE FIGURES 1 AND 2).

6. REINSTALL DOOR TRIM PAD. MAKE SURE SEVILLE DOOR TRIM PADS DO NOT INTERFERE WITH WINDSHIELD GARNISH MOLDING WHEN REPLACING.

#### PARTS INFORMATION:

ELDORADO/SEVILLE - P/N 3548177 (14 NEEDED PER CAR)

PARTS ARE CURRENTLY AVAILABLE THROUGH GMSPO.

#### WARRANTY INFORMATION:

FOR VEHICLES REPAIRED UNDER WARRANTY, USE:

LABOR OPERATION NUMBER: C3348/58 (FRONT DOOR) C3540/41 (REAR DOOR) USE PUBLISHED LABOR TIME. ADD 0.2 HR TO REPLACE CLIPS AND INSTALL FOAM TAPE.

FIGURES: 02 ATTACHMENTS: 00

FIGURE 1:

1. TRIM PANEL 2. SCREW 3. TRIM PANEL RETAINING HOOK

FIGURE 2:

1. TRIM PANEL 2. SCREW 3. TRIM PANEL RETAINING HOOK

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1995 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.