Low Line Pressure. Cadillac Concours 1996

For 1990-2009 cars

Checks | Causes
--- | ---
DEFINITION: Inadequate Lube or Low Line Pressure
Calibration | Incorrect platform or level
Cooler Lines | Clogged or restricted
Lower Channel Plate | Warpage
PCS | Leaking
Pressure Reg. Valve | Stuck due to sediment
Primary Pump Body | Leakage at the gasket or pump body
Scavenge Pipe | Restriction
Scavenge Pipe Seal | Damaged, cut or leaking
Scavenge Pump Body | Leakage at the gasket or pump body
Scavenge Screens | Clogged
Secondary Pump Body | Leakage at the gasket or pump body
Transmission Fluid | Low level