Forward Clutch Plate Assembly and Low and Reverse Band Removal. Cadillac Concours 1997

For 1990-2009 cars

#### Tools Required

J 39053 Forward and Coast Clutch Assembly Puller

1. Rotate the transmission so that the forward clutch assembly (626-834) faces up.
2. Remove the two 13-mm forward clutch support bolts (5) from the case.

Caution: The forward and coast clutch assembly weighs approximately 50 lbs. Personal injury may result if you drop the assembly.

3. Install the J 39053 . Using a chain hoist or suitable lifting equipment, secure and lift the forward and coast clutch assembly (626-834) out of the case.
4. Remove the fretting ring (835).
5. Remove the Lo and Reverse band (13).