Reverse Clutch Housing and Second Sprag Disassemble. Cadillac Concours 1996

For 1990-2009 cars

#### Tools Required

J 39694 Spring Compressor

1. Remove the spiral snap ring (519). Discard the snap ring, which is not reusable.
2. Remove the following parts:

• | The sprag clutch retainer (518)

• | The second sprag outer race

• | The second sprag clutch (516-517)

• | The second sprag outer race thrust washer (520)

Important: Some models will have a reverse clutch pack consisting of a belleville plate (514), three steel plates (511), three fiber clutch plate assemblies (513) and a backing plate (512) with identification marks of A, B or C.

Some models will have a reverse clutch pack consisting of a waved plate (514), two steel plates (511), two fiber clutch plate assemblies (513) and a backing plate (512) with identification marks of 1, 2 or 3.
3. Remove the following parts:

• | The reverse clutch snap ring (515)

• | The reverse clutch backing plate (512)

• | All of the fiber (513) and steel (511) clutch plates

• | The reverse clutch belleville plate (514)

4. Install the J 39694 spring compressor and compress the spring and retainer assembly (509). Then remove the snap ring (510).
5. Remove the following parts:

• | The snap ring retainer (509)

• | The spring and retainer assembly (508)

• | The piston assembly (505)