Idle Air Control Valve Replacement. Cadillac Concours 1996

For 1990-2009 cars

### Removal Procedure

1. Remove the IAC Valve (1) electrical connector.
2. Remove the two IAC valve attaching screws (4).
3. Remove the IAC valve (1) from the throttle body.

### Installation Procedure

1. Install the new IAC O-ring.
2. Install the IAC valve (1) to the throttle body and tighten the screws (4).

Tighten
Tighten the screws to 2.3 N·m (20 lb in).

3. Connect the IAC valve electrical connector.