Cooling System Components. Cadillac Concours 1996

For 1990-2009 cars

Name | Location | Locator View | Connector End View | Group No.
--- | --- | --- | --- | ---
Cooling Fan Motor, LH | Behind the LH side of the radiator | 8A-201-3 Fig 7 | -- | 1.055
Cooling Fan Motor, RH | Behind the RH side of the radiator | 8A-201-3 Fig 7 | -- | 1.055
Cooling Fan Relay #1 | Rearward of the radiator, center bottom between the cooling fans | 8A-201-3 Fig 7 | -- | 1.055
Cooling Fan Relay #2 | Rearward of the radiator, center bottom between the cooling fans | 8A-201-3 Fig 7 | -- | 1.055
Cooling Fan Relay #3 | Rearward of the radiator, center bottom between the cooling fans | 8A-201-3 Fig 7 | -- | 1.055
Engine Compartment Fuse/Relay Center | Forward of the LH front strut tower | 8A-201-21 Fig. 15 | -- | --
Maxi® Fuse Block, RH | Forward of the LH front strut tower, near the engine compartment fuse/relay center | 8A-201-7 Fig. 15 | -- | --
Powertrain Control Module (PCM) | LH front corner of the engine compartment, under the air cleaner housing | 8A-201-4 Fig. 10 | -- | 3.670
C2 (80 cavities) | Engine harness to the PCM, LH front corner of the engine compartment, under the air cleaner housing | -- | 6-Engine Controls | --
G107 | Lower LH front of the engine, below the thermostat housing | 8A-201-19 Fig 38 | -- | --
S117 | Engine harness, about 34 cm (13.4 in) from the RH engine cooling fan connector | 8A-201-3 Fig 7 | -- | --
S118 | Engine harness, about 16.5 cm (6.5 in) from the PCM connector breakout | 8A-201-19 Fig 38 | -- | --
S129 | Engine harness, about 4 cm (1.6 in) from C129 connector breakout | 8A-201-3 Fig 7 | -- | --
S130 | Engine harness, about 6.5 cm (2.6 in) from the EBTCM connector breakout | 8A-201-3 Fig 7 | -- | --