Reaction Carrier/Shell and Third Clutch Installation. Cadillac Concours 1997

For 1990-2009 cars

1. Inspect the reaction shell (633) for damage or wear.
2. Install the reaction shell (633) into the forward clutch housing, with the small teeth facing down.

Note: Following installation, the reaction carrier teeth must seat in the reaction shell.

3. Install the third clutch housing and reaction carrier assembly (604/623) into the case. Twist the housing to install and to insure proper seating.