Evaporative Emission Canister Purge Solenoid. Cadillac Concours 1996

For 1990-2009 cars

### Removal Procedure

1. Remove the intake manifold top cover.
2. Remove the EVAP canister purge solenoid connector (1).
3. Remove the canister purge solenoid vaccum lines.
4. Remove the canister purge (2) solenoid valve bolt.

### Installation Procedure

1. Install the canister purge solenoid (2) valve bolt.

Tighten
Tighten the bolt to 12 N·m (106 in lb).

2. Install the canister purge solenoid vaccum lines.
3. Install the EVAP canister purge solenoid connector (1).
4. Install the bolt.
5. Install the intake manifold top cover.

Tighten
Tighten the bolt to 2 N·m (18 in lb).