For 1990-2009 cars

# WIRE WHEEL COVER FIT (RATTLES) NEW DESIGN WHEEL COVERS

#### SUBJECT: WIRE WHEEL COVER FIT (REPLACE WHEEL COVERS-WHICH INCORPORATES RUBBER INSULATOR)

#### VEHICLES AFFECTED: 1991 'D' MODEL

Some 1991 Broughams (built between VIN sequence numbers 710000 and 713300) may experience an objectionable gap between the wheel trim flange and the wheel cover. This condition may be caused by a poor fit between the wheel cover anti-rotation clips and the wheel.

To repair this condition replace the wheel covers with P/N 10172916 which incorporates a rubber insulator. The centre medallions are to be transferred from the original car.

Use the most applicable Labour Operation and Time from the Canadian Labour Time Guide.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.