For 1990-2009 cars

# REVISED FRONT WHEEL ALIGNMENT SPECIFICATIONS

#### MODELS AFFECTED: 1985-1988 BROUGHAMS

The front wheel toe and camber specifications for 1985-1987 Broughams have been revised. These specifications will also apply to the 1988 Brougham. Use the specifications shown below whenever adjusting front wheel alignment.

SET TO ITEM SPEC.* TOLERANCES ---- ------ ---------- CAMBER 0.0 DEG. +/- 0.50 DEG.

CROSS-CAMBER 0.0 DEG. +/- 1.00 DEG. (LH MINUS RH)

CASTER +3.00 DEG. +/- 1.00 DEG.

CROSS-CASTER 0.0 DEG. +/- 1.00 DEG. (LH MINUS RH)

TOE 0.0 DEG. +/- 0.10 DEG. PER WHEEL

SUM TOE** 0.0 DEG. +/- 0.20 DEG.

* VEHICLE SPECIFICATIONS ARE GIVEN FOR A VEHICLE AT CURB WEIGHT WITH A FULL TANK OF FEUL OR EQUIVALENT COMPENSATING WEIGHT.

** 1/8" SUM TOE IS EQUIVALENT TO AN ANGLE MEASUREMENT OF .12 DEG. PER WHEEL

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.