For 1990-2009 cars

# A/C EVAPORATOR CASE DRAIN DRIP INSTALL NEW DRAIN TUBES

#### SUBJECT: WATER LEAKS/DRIPS INTO PASSENGER SIDE FRONT COMPARTMENT (INSTALL NEW RUBBER DRAIN TUBE)

#### MODELS AFFECTED: 1993 FLEETWOOD BROUGHAMS

Some 1993 Fleetwood Broughams built before VIN breakpoint PR700785 may experience condensate water leaking into the passenger compartment (passenger side front floor area).

This may be found under conditions of extreme humidity when the air flow through the engine compartment can allow a small amount of condensate water to work past the seal of the evaporator drain tube. The water then could slowly drip or seep into the passenger side front compartment, generally wetting the carpet on the floor area near the transmission hump.

#### NOTE: If there is a large volume of water or any leakage noticed in the back seat, use normal diagnostic procedures to determine cause of the leak.

To correct this condition inspect the evaporator drain tube for blockage and clear as required. Install the 90' rubber drain tube over the existing tube, pointed downward, as illustrated. This will allow the water to drain down and away from the evaporator drain opening.

Part Number: 22542866 Part Name: Hose - A/C

Parts are currently available from GMSPO.

For warranty purposes use Labor Operation T7985 at .2 hour.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.