For 1990-2009 cars

# DIRT BUILD-UP ON ROCKER AND LOWER INBOARD DOOR SURFACE

#### SUBJECT: DIRT BUILD-UP ON ROCKER AND LOWER INBOARD DOOR SURFACE

#### MODELS: 1992-94 BUICK ROADMASTER 1992-94 CADILLAC FLEETWOOD 1991-94 CHEVROLET CAPRICE 1991-92 OLDSMOBILE CUSTOM CRUISER

#### CONDITION:

SOME OWNERS MAY EXPRESS DISSATISFACTION WITH MUD COLLECTED ALONG INSIDE BOTTOM OF FRONT DOOR AND ROCKER.

#### CORRECTION:

INSTALL NEW FOAM SEAL, P/N 10249066, (WHEN ORDERING TWO (2) PIECES ARE REQUIRED), ONE FOR LEFT HAND FRONT DOOR AND ONE FOR RIGHT HAND FRONT DOOR. FOLLOW PROCEDURES LISTED BELOW FOR INSTALLATION:

1. WITH THE FRONT DOORS FULLY OPEN, CLEAN THE INSIDE DOOR SURFACE JUST FORWARD OF THE FRONT INBOARD DRAIN HOLE USING ONE OF THE FOLLOWING ADHESIVE CLEANERS:

3M*: GENERAL PURPOSE ADHESIVE CLEANER P/N 08984 AMERICAN SURE SEAL*: URETHANE CLEANER P/N CUSH KENT*: ACRYSOL 20005

2. AFTER CLEANING WITH ABOVE, WIPE CLEAN WITH 50/50 SOLUTION OF ISOPROPYL ALCOHOL AND WATER.

3. SURFACE SHOULD BE 65 DEGREES FAHRENHEIT (18 DEGREES CELSIUS) OR HIGHER.

4. REMOVE PROTECTIVE BACKING FROM FOAM SEAL P/N 10249066.

5. ALIGN THE FOAM SEAL VERTICALLY TO THE FRONT LOWER DOOR SURFACE AND INSTALL IT JUST FORWARD OF THE FRONT DRAIN HOLE. (SEE ILLUSTRATION.) AFTER INSTALLATION, PRESS SEAL FIRMLY TO FULLY SEAT THE SEAL TO THE DOOR.

#### NOTE: IN SOME CASES IT MAY BE NECESSARY TO ADJUST THE DOOR INBOARD SO THAT THE LOWER AUXILIARY CONTACTS THE ROCKER.

*WE BELIEVE THESE SOURCES AND THEIR EQUIPMENT TO BE RELIABLE. THERE MAY BE ADDITIONAL MANUFACTURERS OF SUCH EQUIPMENT. GENERAL MOTORS DOES NOT ENDORSE, INDICATE ANY PREFERENCE FOR OR ASSUME ANY RESPONSIBILITY FOR THE PRODUCTS OR EQUIPMENT FROM THESE FIRMS OR FOR ANY SUCH ITEMS WHICH MAY BE AVAILABLE FROM OTHER SOURCES.

#### PART AVAILABILITY:

PARTS ARE EXPECTED TO BE AVAILABLE ON 2/07/94 FROM GMSPO.

#### WARRANTY INFORMATION:

FOR VEHICLES REPAIRED UNDER WARRANTY, USE: LABOR OPERATION: T-3358 LABOR TIME: 0.3 HR. (FOR BOTH SIDES)

FIGURES: 1

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1994 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.