For 1990-2009 cars

# SQUEAK/CRUNCHING NOISE FROM INSIDE FRONT SEAT BACK

#### SUBJECT: SQUEAK OR CRUNCHNG NOISE INSIDE FRONT SEAT BACK

#### MODELS AFFECTED: 1989-1990 FLEETWOOD SIXTY SPECIALS

Some 1989-1990 Fleetwood Sixty Specials may experience a squeak or crunching noise coming from the front seat back cushions when pressure is applied to the back. To repair this condition use the following procedure:

1. Remove front seat back panel as outlined in Section 10-10-19 of the 1990 Service Information Manual.

2. Disengage and remove both clips holding the trim cover to the seat frame horizontal wires. Refer to Figure 1.

3. Apply a strip of black friction tape over the frame wire at the clip areas. Refer to Figure 1. 4. Reinstall clips over the friction tape. Spread the clip to achieve proper fore and aft movement of the clip on the wire frame and prevent the squeak or crunching noise.

5. Reinstall seat back panel.

For warranty purposes use Labor Operation T6476 at .2 hour for the right and T6475 at .2 hour for the left.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.