For 1990-2009 cars

# RATTLING SOUND APPARENT AT LEFT OR RIGHT HEAD RESTRAINT

#### MODELS AFFECTED: 1989-1990 FLEETWOOD SIXTY SPECIALS

Some 1989-1990 Fleetwood Sixty Specials may experience a "rattling sound" at the left or right head restraint assembly.

To repair this condition use the following procedure:

1. Remove seat back trim panel.

2. Remove drive cable and gear.

3. Remove head restraint and disconnect hose.

4. Remove shaft retainer.

5. Separate shaft retainer and cement two pieces of Velcro material (pile side only) into housing as shown in Figure 1.

6. Reinstall parts as required.

For warranty purposes use Labor Operation T6421 at .3 hour for left and T6422 at .3 hour for right headrests.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.