For 1990-2009 cars

### Removal Procedure

1. Disconnect the electrical connector from the AIR pump (2).
2. Remove the outlet (5) and inlet (4) hoses from the AIR pump (3).
3. Remove the Air pump mounting bolts (3) from the bracket.
4. Remove the Air pump (2).

### Installation Procedure

1. Install the AIR pump (2) to bracket.
2. Install the mounting bolts (3).

Tighten
Tighten the AIR Pump Bolts to 5.6 N·m (50 lb in).

3. Connect the outlet (5) and inlet (4) hoses to the AIR pump (3).
4. Connect the electric connector to AIR pump (3).
5. Check the AIR system for proper operation.