For 1990-2009 cars

# SERVICE REPLACEMENT TRANS ASSY (SRTA) PART NUMBERS

#### SUBJECT: SERVICE REPLACEMENT TRANSMISSION PART NUMBERS - 4T60 (440-T4), THM 200-4R, 3T40, 4T60-E, 4

This bulletin supersedes DSIB 91-1-4 which should be discarded.

The following SRTA unit part number list indicates what model numbers are available from GMSPO and which units they replace. A description of the application is provided where possible.

#### NOTES:

o All SRTA units are designed and remanufactured to current engineering specifications.

o SRTA models should only be considered when the projected cost of repair exceeds the cost of a SRTA replacement.

o Cooler flushing must be performed whenever a transmission is removed for service.

#### IMPORTANT: Beginning with the 1990 model, GMSPO does not automatically consider every SRTA order "VIP" status. To expedite delivery you must specify "VIP" on your order, regardless of model year.

SRTA MODEL REPLACEMENT CHART

#### Hydra-Matic 4T60-E

#### Model Model(s) SRTA Description Year(s) Replaced Model P/N ------------- ------- -------- ----- ------- C 1991 1AVW 1AVW 8651959 C (Limo) 1991 1AZW 1AZW 8651953 C (Export) 1991 1AHW 1AHW 8651957 E/K 1991 1AMW 1AMW 8651952 E/K (Touring) 1991 1AYW 1AYW 8651960 Option GX3 E/K (Export) 1991 1APW 1APW 8651958

#### Hydra-Matic 4T60 (THM 440-T4)

#### Model Model(s) SRTA Description Year(s) Replaced Model P/N --------------- --------- ------------- ----- ------- 4.1L C and Limo 1985-1987 5AF, 5AM, 5AY, 7ALH 8658945 6AF, 6AJ, 6AM, 6AP, 6AS, 7AL 4.1L C Touring 1986-1987 6AC, 6AW, 7AC 7ACH 8658941

4.1L C (Export) 1985-1987 5AR, 6AN, 6AR, 7ARH 8658946 7AR 4.1L E/K 1986-1987 6AA, 6AB, 6AX, 7AHH 8658944 6AY, 7AH 4.1L E/K (Export) 1986-1987 6AD, 6AT, 7AD 7ADH 8658942

4.3L Diesel C 1985 50B 50BH 8658908

4.3L Diesel C 1985 50Y 50YH 8658909

4.5L E/K/C 1988-1990 8AB, 8AA, 9AB, 0KDH 8676900 9AD, 9AA, 9AC, 0AB, 0KD, 0AA, 0KC 4.5L E/K (Touring) 1988-1990 8AJ, 9AJ, 0AJ, 0KHH 8676901 Option GX3 0KH

4.5L E/K (Export) 1988-1990 8AT, 8AN, 9AT, 0KLH 8676902 9AN, 0AT, 0AN, 0KL

4.5L C Limo 1988-1990 8AF, 9AF, 9AH, 0KPH 8676903 0AF, 0KP

Hydra-Matic 4L60 (T-HM 700-R4)

#### Model Model(s) SRTA Description Year(s) Replaced Model P/N ----------- -------- --------- ------ -------- 5.7L D 1990 0DBM 0DBM 8671983

5.7L D 1991 1DBM LDBM 8673910

5.0L D 1991 1DAM 1DAM 8673909

THM 2004R

#### Model Model(s) SRTA Description Year(s) Replaced Model P/N ------------- --------- ------------- ------- --------- 4.1L V6 C 1982-1983 2BY, 3BY 4BY 8639972

RWD C and D 1982-1985 2AA, 3AA, 4AA, 6AA 8669925 5AA California 1985 5AC 6AB 8669926

High alt. 3.73 ratio 1982-1985 2AP, 3AP, 4AP, 6AP 8669927 5AP 2.73 axle ratio 1986 6KC 6KC 8669934

2.73 axle ratio 1987 7KC 7KC 8669924

2.93 axle ratio 1988-1990 8KT, 9KT, 0KT 0KT 8669907

2.73 axle ratio 1990 0KD 0KD 8669902

3.23 axle ratio 1987-1990 7KJ, 8KJ, 9KJ, 0KJ 8669906 0KJ

Hydra-Matic 3T40 (THM 125C)

#### Model Model(s) SRTA Description Year(s) Replaced Model P/N -------------- ---------- ------------- ----- ------- 1.8L J, 2.0L J 1982-1983 2CI, 2CU, 3CB 3CB 8660938

2.0L J 1983 3CA 3CA 8660937 high alt. 2.0L J 1984-1986 4CB, 5C3, 5CB, 6CB 8660911 5CI, 6CB, 6CM 2.0L J 1984-1986 4CA, 5C4, 5CA, 6CA 8660910 high alt. 5CC, 6CA, 6CC 2.8L J 1985-1986 5CJ,6CJ 6CJ 8660913

2.8L J 1987-1988 7CJ,8CJ 9CJ 8665964

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.