For 1990-2009 cars

# CADILLAC SERVICEMAN BULLETIN UPDATES

THE LISTED SERVICEMAN BULLETINS REQUIRE THE FOLLOWING CORRECTIONS. PL EASE UPDATE YOUR BULLETINS TO INCLUDE THESE CHANGES. SERVICEMAN BULLETIN CORRECTION BULLETIN NO: T-87-13 ON THE CHART ON PAGE 1, FILE IN GROUP: 6A FOR THE 1987 ALLANTE, NUMBER: 81 PART NUMBER 3634700 ADD DATE: SEPT. '86 NOTE: INCLUDES IGNITION DISTRIBUTOR BULLETIN NO: T-87-36 PAGE 2, STEP 13 SHOULD READ: FILE IN GROUP: 3D HOSE CLAMP OVER GROOVED AREA NUMBER: 7 OF AIR BLADDER AND TIGHTEN DATE: NOV. '86 SECURELY, SEE FIGURE 10. BULLETIN NO: T-87-52 ON PAGE 2 IN THE FILE IN GROUP: 7 ILLUSTRATION, THE PART NUMBER: 151 NUMBER FOR THE CUP PLUG DATE: DEC. '86 SHOULD BE CHANGED FROM 8646984 TO 8646987 BULLETIN NO: T-87-60 IN FIGURE 1, USE BOLT FILE IN GROUP: 6B 11504299 TOGETHER WITH NUMBER: 15 1052624 THREAD LOCK DATE: JAN. '87 ADHESIVE INSTEAD OF 1637233 BULLETIN NO: T-87-93 IN PARAGRAPH 1 DELCO BOSE FILE IN GROUP: 9 RADIO OPTION IS LISTED AS NUMBER: 36 OPTION CODE VQ4 THE COR- DATE: APR. '87 RECT CODE IS UQ4. (CADILLAC DISCLAIMER)

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.