For 1990-2009 cars

# MANUAL SEAT BACK RECLINER MOVEMENT

#### VEHICLES AFFECTED: 1987-1989 C/H

Some 1987-1989 C and H cars equipped with manual seat back recliners may experience slight seat back movement.

To repair this condition replace the recliner assembly with the part numbers listed below:

Recliner Recliner Kit Kit Application (H-Car) (C-Car)

12501267 12501269 ............... Coupe Recliner - Passenger 12501268 12501270 ............... Coupe Recliner - Driver

12501271 12501273 ............... Sedan Recliner - Passenger 12501272 12501274 ............... Sedan Recliner - Driver

#### IMPORTANT: Each recliner kit contains a recliner and four bolts.

Refer to the appropriate Service Information Manual, Section 10-9, for the installation procedure.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.