For 1990-2009 cars

# ADJUSTING TIRE PRESSURE DURING NEW VEHICLE PREP

Currently, all tires are shipped to dealers at tire pressures from 35-41 psi. The pressures are set higher at the plant primarily to assure proper bead seating. The processing pressures may be higher than the customer recommended pressures. Refer to Figure 1.

Recently we have received several comments of harsh ride which have been traced back to tire pressures. The tire pressures of these cars had not been adjusted to the tire placard specifications as required during NVI-PDI.

As part of the new car delivery process (NVI-PDI), the tire pressures are to be adjusted to the recommended tire pressure as specified on the tire placard to reduce harsh ride condition. To assure customer satisfaction it is important that the tire pressures be properly adjusted before new car delivery.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.