For 1990-2009 cars

# FLASH-TO-PASS USES LOW BEAMS INSTEAD OF HIGH BEAMS

#### SUBJECT: FLASH-TO-PASS USES LOW BEAMS INSTEAD OF HIGH BEAMS (REWIRE CONNECTOR)

#### MODELS: 1993 CADILLAC FLEETWOOD BROUGHAM 1994-96 CADILLAC FLEETWOOD

#### CONDITION:

SOME OWNERS MAY COMMENT THAT THE FLASH-TO-PASS FEATURE USES THE LOW BEAMS RATHER THAN THE HIGH BEAMS. FOR 1993 TO 1995, FLASH-TO-PASS WAS NOT AVAILABLE ON CANADIAN VEHICLES WITH DAYTIME RUNNING LIGHTS (DRL).

#### CAUSE:

THE TERMINALS IN THE CONNECTOR TO THE HEADLIGHT DIMMER SWITCH WERE REVERSED. THIS WAS CORRECTED FOR 1996 PRODUCTION ABOUT SEPTEMBER 26, 1995.

#### CORRECTION:

LOCATE THE CONNECTOR TO THE HEADLAMP DIMMER SWITCH ON THE LEFT SIDE OF THE STEERING COLUMN. UNPLUG THE CONNECTOR, THEN REMOVE TERMINALS A AND C AND REINSTALL IN THE OPPOSITE CAVITIES. PLUG THE CONNECTOR BACK IN, THEN CHECK TO MAKE SURE THE HIGH BEAMS COME ON WITH FLASH-TO-PASS.

#### IMPORTANT: IF A DAYTIME RUNNING LIGHT (DRL) KIT IS ADDED TO THE VEHICLE, MAKE SURE TO PERFORM THIS PROCEDURE TO INSURE PROPER OPERATION OF THE DRL SYSTEM. SEE BULLETIN #53-82-09.

#### WARRANTY INFORMATION:

FOR VEHICLES REPAIRED UNDER WARRANTY, USE:

LABOR OPERATION NUMBER: N6360 USE PUBLISHED LABOR OPERATION TIME.

FIGURES: 00 ATTACHMENTS: 00

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1995 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.