For 1990-2009 cars

# SWITCH PLATE RETAINER REPAIR FRONT DOOR WINDOW

IF A CONDITION IS ENCOUNTERED WHERE THE DOOR WINDOW SWITCH PLATE RETAINER AND/OR CLIP IS BROKEN, IT MAY BE REPAIRED AS FOLLOWS: 1. REMOVE SWITCH PLATE FROM DOOR ARMREST ASSEMBLY. 2. CLAMP SWITCH PLATE FACE DOWN IN VISE. NOTICE: CENTER SWITCH PLATE BETWEEN TWO (2) PIECES OF WOOD TO AVOID DAMAGING SWITCH PLATE FINISH. 3. FILE OR GRIND RETAINER ATTACHING STUD(S) UNTIL SMOOTH. 4. CENTER PUNCH SWITCH PLATE STUD(S) PRIOR TO DRILLING. 5. USING A 3/32" (2.75MM) DRILL WITH A DRILL STOP SET AT 9/32" (7MM), DRILL HOLE(S) AT LOCATIONS SHOWN IN FIG. 1. 6. INSTALL RETAINER AND/OR CLIP WITH A SELF-TAPPING PANHEAD #4 MACHINE SCREW(S) AS SHOWN IN FIGURE 1. 7. CONNECT WIRING AND INSTALL SWITCH PLATE TO DOOR ARMREST. 8. CHECK SWITCH FOR PROPER OPERATION.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.