For 1990-2009 cars

# CADILLAC SERVICEMAN BULLETINS UPDATES & CORRECTIONS NOTED

#### MODELS AFFECTED: 1985-86 DE VILLES AND FLEETWOODS 1985-86 CIMARRONS 1984-85 BROUGHAMS, ELDORADOS AND SEVILLES

The listed Serviceman Bulletins require the following corrections. Please update your bulletins, to include these changes.

Service Bulletin Correction -------- ---------- Bulletin No. T-86-3 Step 3 should read: File in Group 10 Loosen primary hood latch Number 73 mounting screws (Figure 2) Date Sept.'85 and lower primary hood Models Affected 1985 De Villes/Fleetwoods latch 1/16".

Bulletin No. T-86-14 Labor Operation K6626 File in Group 7 should be changed Number 127 from .3 to .5 hours. Date Nov.'85 Models Affected 1985-86 De Villes/Fleetwoods

Bulletin No. T-86-31 The first paragraph under File in Group 7 Warranty Information should Number 129 be changed to read: On 1985 Date Feb.'86 models, use Labor Operation Models Affected 1985-86 Cimarrons K6300 for .5 hours (includes replacing the convertor cover and three converter to flexplate bolts).

Bulletin No. T-86-40 Under Description and Part File in Group 3B Numbers: 3/8" Hose Clamps Number 17 (2 required) P/N 22527583 Date Mar. '86 should be P/N 25518880 Models Affected 1985 De Ville/Fleetwood

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.