For 1990-2009 cars

# MOTOR VEHICLE REGISTRATION DATA

1984 Cadillac Motor Vehicle Registration Data

Cadillac Vehicle Description - Weights - Wheelbase - Engine Data

V.I.N. Body Body No. Engine Shipping Weight Series Name Designator Type Pass Code Kilograms Pounds ----------- ---------- ---- ---- ---- --------- ------ Fleetwood W-47 2-door 8 1755.0 3869 Brougham Coup Coupe N 1904.3 4198

Fleetwood W-69 4-door 8 1774.6 3912 Brougham Sedan Sedan 6 N 1931.4 4258

Deville M-47 2 door 8 1732.2 3819 Coupe Coupe N 1881.5 4148

Deville M-69 4 door 8 1751.1 3861 Sedan Sedan N 1907.1 4204

Fleetwood F-23 4 door 8 9 2106.1 4642 Limousine Sedan 7 Fleetwood F-33 2146.7 4730 Formal Limousine Commercial Z-90 6 Chassis Eldorado Coupe L-57 2 door 6* 8 1645.4 3627 Coupe N 1803.7 3976

Eldorado L-67 2 door 8 8 1726.5 3806 Biarritz Convertible Coupe Seville Sedan S-69 4 door 6* 8 1677.1 3697 Sedan N 1835.4 4046 Cimarron Sedan G-69(STD)*4 door P 1140.5 2514 G-89(OPT)**Sedan 5 P 1158.0 2552

Wheelbase Engine CU. IN. Series Name Millimeters Inches Displacement ----------- ----------- ------ ------------- Fleetwood V8-250 CU IN Digital Brougham Coup Fuel Injection (DFI)

Fleetwood Brougham Sedan 3085 121.5 V8-350 CU IN Diesel- Not Available in California Deville Or On Eldorado Biarritz Coupe Convertibles, Eldorado Touring Coupes Deville Limousines or Sedan commerical Chassis

Fleetwood V8 6 4 -358 CU In Digital Limousine 3670 144.5 Fuel Injection (DFI)- Fleetwood Fleetwood Limousine Only Formal Limousine Commercial Chassis Eldorado Coupe V8-368 CU IN 4 Barrel Carburetor Commercial Eldorado 2895 114.0 Chassis Only Biarritz Convertible Seville Sedan

Cimarron Sedan 2571 101.2 L4-121 CU IN Eectronic Fuel Injection (EFI)

* Manual Transmission ** Automatic Transmission

All weights include automatic transmission (manual transmission on Cimarron), power steering, power brakes, and air conditioning which are standard on all vehicles Weights estimated for non-California vehicles at time of publication. Production weights may vary slightly. Please Note: Taxable horsepower is 46.2 for the 368 CU IN engine. 52.7 for the 350 CU IN engine, 19.6 for the 121 CU.IN. engine, and 36.4 for the 250 CU.IN engine. See engine codes below *Eldorado Touring Coupe and Seville Elegante passenger capacity is five.

#### Engine Specifications

Displacement Cylinder Net Horsepower Fuel Engine CU.IN. Liters Arrangement (SAE J-245) System Code ------ ------ ------------ ----------- ------ ---- 250 4.1 V-8 Digital Fuel Digital 8 Injection 101(KW) Fuel 135 HP Injection

121 2.0 L-4 Electronic Fuel Electronic P Injection 66 Fuel Injection (KW) 88 HP 350 5.7 V-8 Diesel 78(KW) Diesel N 105 HP

366 6.0 V-8/6/4 Modulated Digital Displacement Fuel Injection 9 Digital Fuel Injection 105 (KW) 140 HP

366 6.0 V-8 Carbureted 112(KW) Carburetor 6 150 HP

Displacement Bore and Stroke CU.IN. Liters Millimeters Inches ------ ------ ----------- ------ 250 4.1 88.0 x 84.0 3.46 x 3.31

121 2.0 89.0 x 80.0 3.50 x 3.15

350 5.7 103.0 x 86.0 4.057 x 3.865

366 6.0 96.5 x 103.1 3.800 x 4.060

366 6.0 96.5 x 103.1 3.800 x 4.060

#### Cadillac Vehicle Identification Number Information

Each 1984 Cadillac automobile or commericial chassis carries a 17-digit vehicle identification number used for license and insurance identification and in general reference to the automobile. The number is located on a plate riveted to the windshield lower frame at the driver's side of the car where it is visible through the windshield. The 1984 Cadillac Vehicle Identificaton is decoded below.

1 = Nation of Origin - 1 Denotes USA

G = Manufacturer - G denotes General Motors

6 = Make "6" denotes Cadillac "E" denotes Dadillac incomplete vehicle

A = Restraint system or GVWR/Brake System Code A - Non Passive restraint E - 6001 lb. to 7000 lb. GVWR range

M = Car line and series M - Brougham L-Eldorado W - Deville (RWD S-Seville F - Limousine G-Cimarron

00 = Body Type

S = Engine code "8" denotes 250 CU IN with digital fuel injection 4.1 liters "N" denotes 350 CU IN diesel 5.7 liters "9" denotes 368 CU IN with digital fuel injection 6.0 liters "6" denotes 368 CU IN with carburetor 6.0 liters "P" denotes 121 CU IN with electronic fuel injection 2.0 liters

X = check Digit

E = Model Year (E-1984)

9 = Assembly Plant 9 Detroit Michigan (D series) E Linden, New Jersey (E&K series) J Janesville, Wisconsin (J series)

000001 = Production sequence number 000001 DM, DW and D - Detroit 6000001E - Linden 800001K - Linden 400001J - Janesville

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.