For 1990-2009 cars

# SERVICE GUILD: ADHESIVE REMOVAL DISCS & EQUIP INFO.

#### SUBJECT: ADHESIVE REMOVAL DISCS AND EQUIPMENT (INFORMATION BULLETIN)

#### VEHICLES AFFECTED: 1983-92 ALL PASSENGER CARS AND TRUCKS

Attached is information on an available Scotch-Brite product for quick, easy removal of adhesives from body side moldings and painted body panels. Required equipment includes a high-speed drill motor along with removal discs and holder.

These products were tested on General motors molding systems and were found to be quick and effective, eliminating the need for solvent adhesive removers and hand rubbing. Since it is recommended that body side moldings be removed carefully and reused whenever possible, this equipment can save time on molding and body clean up.

#### CAUTION:

Always wear protective eye wear and/or face shield when operating equipment of this type as particles may become airborne.

We believe this source and their equipment to be reliable. There may be additional manufacturers of such equipment, however, General Motors does not endorse, indicate any preference for, or assume any responsibility for the products or equipment from these firms or for any such items which may be available from other sources.

#### SCOTCH-BRITE MOLDING ADHESIVE AND STRIPE REMOVAL DISCS

The Best Way Yet to Remove Vinyl Decals, Graphics, Striping Tapes and Molding Adhesive

Scotch-Brite Molding Adhesive and Stripe Removal Discs are fast and easy to use. The unique construction of the discs assures long life and allows easy conformability to contours. Because the discs are flexible and have no sharp edges, they will not damage underlying paint. Not recommended for use on acrylic lacquer paints.

The discs are faster and cleaner than solvent or chemical adhesive removers and are non-combustible as well.

- Won't scratch the paint surface - will not damage acrylic enamel or urethane paint.

- Fast, safe and easy to use - -faster, safer and easier to use than solvents or adhesive cleaners and there's never any fire danger because the discs are non-combustible.

- Long lasting - unique construction provides optimum disc life.

- Flexible - removes decals, graphics, striping tape and molding adhesive from irregular surfaces and contours.

- Produced in a circular disc form - product has no sharp edges to cause damage to surface.

#### Important: Disc must be run on tools that have proper speed and torque ratings.

#### Scotch-Brite" Molding Adhesive and Stripe Removal Discs

The fastest, most economical way to remove vinyl decals, graphics, striping tapes and molding adhesive without damaging underlying paint.

Scotch-Brite Molding Adhesive Stripe Removal Discs are available in two sizes: ------------------------------------------------------------------------------ 4-inch Discs (Part No. 07501) ----------------------------- - Recommended for vinyl decals, graphics, striping tapes and molding adhesive left on car.

- Required tool speed - 4,000 RPMs

6-inch Discs (Part No. 07502) ----------------------------- - Recommended for large adhesive areas requiring removal. May also be used on bench motor to remove adhesive from backside of molding.

- Required tool speed - 2,800 RPMs

Exclusive Roloc + Holder System is fast and easy to use. -------------------------------------------------------- The Roloc + Holder allows you to use Scotch-Brite Molding Adhesive and Stripe Removal Discs on your tool. The Roloc + Holder is quick and easy to use and will save you time and money. The 1/4-inch shank fits into any recommended standard tool. A simple twist and the disc is attached and ready to use!

#### Suggestions for Proper Operation

1. Properly tighten holder in collet or chuck of portable tool.

2. Twist disc assembly into the holder. Be certain assembly is securely tightened.

3. With tool running, bring outer edges of discs into contact with material to be removed. Light contact pressure is all that is needed.

4. Guide the tool so that the tool is working counter to the directional rotation of the disc.

#### Ordering Information

#### Scotch-Brite- Molding Adhesive and Stripe Removal Discs

Part No. Size Discs/Bag Bags/Case -------- ---- --------- --------- 07501 4 in. x 3/8 in. 1 5 07502 6 in. x 3/8 in. 1 5

Roloc + Holder -------------- Part No. Size Quantity/Case -------- ---- -------------- 07500 1 in. diameter / 1/4 in. shank 1

#### CAUTION

------- Always use protective eye wear and/or face shield as recommended ANSI Standard Z87.1

#### MOS (Maximum Operating Speed)

DO NOT EXCEED! 4,500 RPM spindle speed for 4-in. diameter 4,000 RPM spindle speed for 6-in. diameter

#### Required Operating Speed

2,000 to 3,000 SFPM (Surface Feet Per Minute) when product is in contact with the work surface. This translates into a 2,000 to 3,000 RPM range for the 4-in. diameter disc and 1,300 to 1,900 RPM for the 6-in. diameter disc.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.