For 1990-2009 cars

# LABOR TIME GUIDE REQUEST FOR REVIEW UPDATE

This bulletin contains information on Labor Time Guide Requests For Review answered from March 3, 1990 to May 29, 1990. In total, 78 answers were sent to dealers. Of these, 59 resulted in increased time allowances or the addition of a new operation. Many of these changes appear in the April LTG revision; all others are summarized on the attached sheets and will be published in the next LTG revision. New operations are indicated as NOP. Time increases are indicated with a +. Special thanks go to all dealers who have submitted Requests For Review. Your participation has really helped improve the quality of the Labor Time Guide. If you have any comments or suggestions, please send them in on a Request For Review form or call Jeff Clark on (313) 554-6946.

LABOR DESCRIPTION YEARS C D E K V OPERATION

B0316/17/19 Strip, Front Bumper Fascia Molding-R&R or Replace 1989-1990 .9 NOP - Right, Left, Center B3710 Lid, Stowage - Replace 1987-1990 .8 +

B3720/21 Extension, Stowage Lid 1987-1990 .2 NOP - Replace B4180/81 Cylinder, Front Door Lock - R&R or Replace 1987-1990 .9 +

B7820/21 Molding, Front Door Window Frame - R&R or Replace 1990 .2 NOP B8680/81 Bezel, Tail Lamp - Replace 1989-1990 .2 NOP

C0070/71 Glass, Front Door Vent 1987-1990 2.0 NOP - Replace C0140 Channel, Front Door Window Run - R&R or Replace 1990 .8 +

C0340/41 Channel, Rear Door Window 1985-1990 .9 + Run - R&R or Replace

C1280 Weatherstrip, Rear Compartment - Align or 1985-1990 .3 NOP Replace 1982-1990 .6 NOP 1986-1990 .5 .5 NOP 1987-1990 .5 NOP

C1500/01 Retainer Weatherstrip 1986-1990 .2 NOP - Align or Replace C2860 Console Assembly 1986-1990 .4 .4 + - R&R or Replace C3348/58 Trim Assembly, Front Door - R&R or Replace 1987-1990 .4 .4 + ADD: with courtesy lamp .1 .1 to transfer carpet .1 .1 panel to transfer finishing molding .2 .1 and/or pull handle .1 .1 to transfer speaker cover D0770 Programmer, Air 1986-1990 .5 .5 + Conditioning - R&R D1328 Motor and/or Fan, Blower - R&R or Replace 1987-1990 1.1 + D2700 Valve, Coolant - Replace 1986-1990 .6 + D4440 Compressor, Assembly 1985-1990 - Replace .7 .7 .7 .7 .7 NOP ADD: recover and recharge

E7200 Cylinder, Ignition Lock 1990 1.3 - R&R or Replace

LABOR OPERATION DESCRIPTION YEARS C D E K V

J0301 Cover and/or Gasket, 1986-1990 .8 + Rocker - Replace J0370 Arm and/or Pivot, 1990 1.3 1.3 + Rocker - Replace J1000 Pan and/or Gasket, 1986-1990 1.4 1.4 + Oil - Replace J1500 Mount, Engine 1985-1990 2.2 + - Replace J1840 Engine, Universal 1986-1990 10.0 + - Replace (Code Y) .2 ADD: with cruise J3176 Line and/or Hose, Engine Oil Cooler - 1990 .5 NOP Replace (One) (Code 7) J3177 Line and/or Hose, Engine Oil Cooler - Replace (Both) (Code 7) 1990 .6 NOP

J3460 Hose and/or Pipe, Thermostat Bypass-Replace .9 NOP

J4080 Generator Assembly 1987-1990 1.1 1.1 1.1 1.1 + - Disassemble, ADD:to R&R bridge, output .2 .2 .2 .2 + terminal nut, regulator, .1 .1 .1 .1 + and brushes to desolder and solder regulator J4100 Generator Assembly 1988-1990 .7 .7 .7 .7 + - Replace ADD: with heated windshield .1 +

J4620 Motor Assembly, Starter 1986 1.3 1.3 + J5650 - R&R Injector, Fuel Replace 1990 1.2 1.2 1.2 + INC: one or all injectors J6410 Motor, Idle Speed Control 1990 .8 + - Replace

K6200 Cable and/or O-Ring, Throttle Valve Control 1989-1990 (TV) - Replace (200-4R) ADD: to oil pressure test .5 NOP K6430 Governor Assembly - R&R 1989-1990 or Replace ADD: to oil pressure test .5 NOP K7000 Transmission Assembly 1989-1990 .5 NOP - Replace ADD: to oil pressure test

L2300 Converter, Exhaust Catalytic 1989-1990 .8 - Replace

N0476 Bulbs, Cornering Lamp 1990 .2 .2 .2 .2 NOP - Replace N4800 Computer (Control), Body 1990 .6 .8 NOP - Replace N4834 Module, Passive Restraint 1990 .2 NOP - Replace

LABOR DESCRIPTION YEARS C D E K V OPERATION R0200 Antenna, Power - R&R 1985-1988 .6 +

R0480 Antenna, Complete 1989 .7 + Assembly - Replace R1000 Mats, Carpet Saver, 1987-1990 .2 NOP One or All - Replace

T6365 Install Weatherstrip 1987-1988 22.5 NOP Kits T6431 Rivet Window Sash 1989 .5 + Channel

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.