For 1990-2009 cars

# LABOR OPERATION C8835 AND E7010

This bulletin has been reprinted because the art work was omitted.

This bulletin is to clarify use of Labor Operations C8835 and E7010. The guidelines below should be followed when servicing the inflator module or horn mechanism on vehicles equipped with Supplemental Inflatable Restraint (SIR).

#### C8835 - Module, Inflatable Cushion:

To be used when replacing the inflator module. Removal and installation to access other serviced parts (i.e., horn mechanism components) does not qualify for usage of this Labor Operation.

E7010 - Emblem and/or Pad, Horn Button: --------------------------------------- To be used when servicing any of the horn mechanism components (see parts illustration). Do not use this Labor Operation when replacement of the inflator module is required.

Your cooperation with these guidelines will ensure accurate product feedback and proper credit for service work performed.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.