For 1990-2009 cars

# FUEL TANK SENDING UNIT INSTALLATION PROCEDURE

#### VEHICLES AFFECTED: 1985 Ninety-Eight

The procedure listed below should be followed when installing a fuel tank sending unit in a 1985 Ninety-Eight.

1. Insert tank sending unit into tank.

2. Hold the sending unit so that the plate of the sending unit is four inches above the ring on the tank.

3. Rotate the sending unit until the front of the fuel sock is pointing forward in the tank.

4. Lower the sending unit until it contacts the ring on the tank.

5. Position the sending unit in its final place and lock with the cam ring.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.