For 1990-2009 cars

# MOUNTING BOLT TORQUE-SPECS. THROTTLE BODY INJECTION

SECTION 0B OF THE 1982-1985 SERVICE INFORMATION MANUALS LIST "THROTTLE BODY MOUNTING BOLT TORQUE" OR "FUEL INJECTION MOUNTING BOLT TORQUE" AS AN EMISSION CONTROL SERVICE ITEM. SOME EDITIONS OF THE 1982-1985 CADILLAC SERVICE INFORMATION DO NOT LIST A TORQUE SPECIFICATION. THROTTLE BODY MOUNTING BOLT TORQUE SPECIFICATIONS ARE AS FOLLOWS: TORQUE 1982-1985 HT4100/DFI 20 N.M/15 FT.-LB. 1983-1985 2.0L/EFI 23 N.M/17 FT.-LB. CHECK APPROPRIATE "SERVICE INFORMATION" MANUAL FOR RECOMMENDED SERVICE INTERVAL.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.