For 1990-2009 cars

# ANTI-LOCK BRAKE WIRING HARNESS REPAIR

ANTI-LOCK BRAKE WIRING HARNESS REPAIR

#### VEHICLES AFFECTED: 1986-88 "C" AND 1987-88 "H" MODELS WITH ------------------ ANTI-LOCK BRAKES

Two new service kits have been released to repair the anti-lock brake wiring harness. Kit Number 12058538 contains a front wheel speed sensor coaxial cable. This kit should be used to replace damaged coaxial cable, connectors and terminals on the harness side of the wheel speed sensors.

Kit Number 12058539 contains a rear wheel speed sensor coaxial cable. This kit should be used to replace damaged wheel speed sensor coaxial cable, connectors or terminals.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.