For 1990-2009 cars

# DRIVER SEAT CANNOT BE ADJUSTED HIGH ENOUGH--CORRECTION KIT

#### SUBJECT: DRIVER'S SEAT CANNOT BE ADJUSTED HIGH ENOUGH (CORRECTION KIT)

#### VEHICLES AFFECTED: 1991-92 "C AND H" MODELS PONTIAC BONNEVILLE OLDSMOBILE EIGHTY EIGHT, NINETY EIGHT BUICK LE SABRE, PARK AVENUE CADILLAC DEVILLE, FLEETWOOD

#### CONDITION:

---------- A condition where the seat may not have enough upward travel may be noted on the subject vehicles.

#### CORRECTION:

----------- 1. Obtain Kit, Part Number 12520796.

2. Remove the four (4) hexhead bolts attaching the seat frame to the adjuster. On vehicles with the 6-way power seat option, the adjuster must be in the full "up" position to remove these bolts.

3. Insert the spacer between the seat frame and adjuster at all four bolt locations. (See Figure 1)

4. Coat threads of the new replacement bolts with thread sealant/adhesive, GM Part No. 12345382, and attach the seat frame to the adjuster.

5. Torque the attaching bolts to 22-28 N.m (17 lbs. ft.).

For vehicles repaired under warranty use:

Labor Time: Left (Driver's Side) 0.8 hour. Right (Passenger's Side) 0.8 hour.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.