For 1990-2009 cars

# NYLON WHEEL WEIGHTS- PART NUMBERS / INSTALLATION

#### MODELS AFFECTED: 1985-1987 FWD DE VILLES AND FLEETWOODS, 1979-1987 ELDORADOS, 1980-1987 SEVILLES, AND 1982-1987 CIMARRONS

Vehicles equipped with aluminum wheets may exhibit a condition of corrosion around some wheel weights. Wheel corrosion can be repaired using the procedure outlined in Serviceman Bulletin T-87-4. Additionally, a new style wheel weight is available to prevent this condition. The new weight is nylon coated and is available from GMWDD using the part numbers listed below.

Weight (oz.) Part Number ------------ ----------- .25 9591358 .50 9591359 .75 9591360 1.00 9591361 1.25 9591362 1.50 9591363 2.00 9591365 2.50 9591367 3.00 9591369

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.