For 1990-2009 cars

# NEW A/C HIGH SIDE PRESSURE SERVICE PORT ASSY. INFORMATION

#### SUBJECT: INFORMATION - NEW A/C HIGH SIDE PRESSURE SERVICE PORT ASSEMBLY

#### VEHICLES AFFECTED: 1991-92 A,C,D,E,F,K,W MODELS

#### Application:

1991-92 Chevrolet Camaro and Pontiac Firebird 1991-92 Chevrolet Lumina 1991-92 Pontiac Grand Prix and 6000 Models 1991-92 Buick Regal and Century 1991-92 Oldsmobile Cutlass Supreme and Ciera 1992 Cadillac DeVille, Fleetwoood, Eldorado, Seville, and Brougham

All 1991-92 "W" and "All models, some interim 1991-92 'IF" models, and 1992 "C", "D", "E", and "K" models equipped with new A/C high pressure service port assembly. The A/C low side pressure service port will remain the same.

Figure 1 1991 and Later Vehicles Figure 2 Older Vehicles

Tool J 38702, is a straight adapter which allows existing diagnostic equipment to be connected to the service port, and high side pressures to be checked by opening the port. The adapter connects, first to the gage hose and then to the high side pressure port, by threading the adapter to the port.

#### IMPORTANT: Tool J-38702 Adapter MUST BE ASSEMBLED to the fitting FINGER TIGHT. Using a tool to tighten this adapter may exceed the assembly torque of the 2 piece High Side Service Port Assembly. If this occurs, the attempted removal of the adapter may result in the service port fitting being removed with it, causing loss of refrigerant.

Tool J 38704, is an octagon socket which is used to unthread the A/C high side pressure port from the high side A/C line and then used to thread the new port back onto the high side pressure line.

Tool J 38702 Tool J 38704 Straight Adapter Octagon Socket

Service parts are as follows:

Part Part Number

Valve Core Housing and 0-ring 52456273

0-ring 52450548

Parts are currently available from CANSPO.

#### CAUTION:

NEVER REMOVE THE GAUGE LINE FROM ITS ADAPTER WHEN THE LINE IS CONNECTED TO THE A/C SYSTEM. ALWAYS REMOVE THE LINE ADAPTER FROM THE SERVICE PORT TO DISCONNECT A LINE. DO NOT REMOVE THE CHARGING HOSE AT THE GAUGE SET WHILE ATTACHED TO THE SERVICE HIGH SIDE PORT. THIS WILL RESULT IN COMPLETE DISCHARGING OF THE SYSTEM DUE TO THE DEPRESSED VALVE AND MAY CAUSE PERSONAL INJURY DUE TO ESCAPING REFRIGERANT.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.