FRONT DOOR GLASS INSTALLATION AND ADJUSTMENT. Cadillac Limousine 1986

For 1990-2009 cars

# FRONT DOOR GLASS INSTALLATION AND ADJUSTMENT

#### MODELS AFFECTED: 1985-86 FWD DE VILLES AND FLEETWOODS

This bulletin revises the procedure outlined in the 1986 Body Service Manual (page 5C-24) for installation of the front door window assembly for the 1985-86 FWD De Villes and Fleetwoods. INSTALL OR CONNECT (Figure 1)

1. Front run channel (2) and screws (1) to door, tighten loosely.

2. Glass lower sash channel to guide on regulator by lowering glass into door from outboard side of door frame and rotating glass until the regulator guide is connected to the glass sash channel.

3. Rear guide (4) on glass to rear run channel (7) by pulling back on glass until rear guide snaps into rear run channel.

4. Front guide on glass to front run channel by reaching through front access hole in door inner. Grasp front run channel and snap onto glass guide, pushing front channel rearward until guide snaps into channel.

#### ADJUST

a. Move glass upward in to door frame header, approximately 5 mm (.20") short of full up position.

b. Grasp door glass and move glass rearward to assure full engagement of glass and glass guide pin to glass run channel and retainer, then move glass fully upward into door header.

c. Tighten previously loosely installed upper and lower glass run channel retainer screws (1) to 11.0 N.m (93 in. lb.).

d. Cycle glass down then to full up position to check operation of glass.

5. Insulator for outside mirror. 6. Outside mirror cover. 7. Inner belt sealing strip and fillers. 8. Trim panel upper retainer. 9. Water deflector. 10. Trim panel.

For warranty purposes, use Labor Operation C0100 (RH) or C0101 (LH) at .5 hours.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.