LOOSE DOOR WINDOW SWITCH PLATE REPAIR PROCEDURE. Cadillac Limousine 1985

For 1990-2009 cars

# LOOSE DOOR WINDOW SWITCH PLATE REPAIR PROCEDURE

#### VEHICLES AFFECTED: ALL 1985 'C' STYLES

#### Notice:

This bulletin supersedes 85-2-128,dated Feb.28,1985. Change made in recommended materials.

If a condition is encountered where the door window switch plate base,it may be repaired as follows:

1. Using 3M-8984, or equivalent solvent, thoroughly clean cementing surfaces.

2. Using 3M-8101 structual adhesive, Loctite Quick Jel (SGGA) or equivalents, recement escutcheon to switch plate base. Follow manufacturer's label directions for bonding.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.