POWER STEERING SYSTEM NOISE NEW POWER STEERING PUMP P/N. Cadillac Limousine 1987

For 1990-2009 cars

# POWER STEERING SYSTEM NOISE NEW POWER STEERING PUMP P/N

#### MODELS AFFECTED: 1987-1988 DE VILLES AND FLEETWOODS WITH BASE SUSPENSION

Some 1987-1988 DeVilles and Fleetwoods with base suspension may exhibit a condition of power steering system noise. This condition may be caused by the power steering pump. To repair this condition a new power steering pump, P/N 26012285, is available for service from GMSPO. The new pump has a reduced flow rate which reduces noise caused by the pump.

1987 and 1988 DeVilles and Fleetwoods with Touring Ride & Handling Suspension (RPO FE2) must still be serviced with power steering pump P/N 26006703. These vehicles have a close ratio, higher effort steering gear that, when used with the new pump, could result in high steering efforts during certain maneuvers.

Refer to Serviceman Bulletin T-87-48, Group 3B, and Section 3 of the appropriate Service Information Manual for power steering noise diagnosis. Refer to Section 3B3 of the appropriate Service Information Manual for power steering pump service procedures. Refer to Serviceman Bulletin T-87-55, Group 3B, for revised power steering system bleed procedure.

For warranty purposes use Labor Operation E9050 at .5 hour.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.