For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
DEFINITION:When the pedal assembly is pressed to the floor, the shift lever does not move freely in and out of reverse gear.
1 | Check for a pedal restriction. Is the vehicle equipped with the aftermarket floor covering? | -- | Go to Step 2 | Go to Step 3
2 | Remove the aftermarket floor covering. Does the clutch work properly? | -- | System OK | Go to Step 3
3 | Check the clutch system. Does the clutch work properly? | -- | System OK | Go to Step 4
4 | Check for loose clutch cover to flywheel bolts. Are the clutch bolts loose? | -- | Go to Step 5 | Go to Step 6
5 | Tighten the clutch cover to flywheel bolts to specifications. Refer to Fastener Tightening Specifications . Does the clutch work properly? | -- | System OK | Go to Step 6
6 | Check the clutch spin down time. Refer to Clutch Spin Down Time . Is the spin down time OK? | -- | System OK | Go to Step 7
7 | Check for air in the clutch hydraulic system. Is there air in the clutch hydraulic system? | -- | Go to Step 8 | Go to Step 9
8 | Bleed the clutch hydraulic system. Refer to Hydraulic Clutch Bleeding . Does the clutch work properly? | -- | System OK | Go to Step 9
9 | Ensure that the clutch disc is not warped or bent. Is the clutch disc warped or bent? | -- | Go to Step 10 | Go to Step 11
10 | Replace the clutch disc. Refer to Clutch Pressure and Driven Plate Replacement . Does the clutch work properly? | -- | System OK | Go to Step 11
11 | Check the master cylinder and actuator for worn seals. Are the seals worn? | -- | Go to Step 12 | Go to Step 13
12 | Repair the necessary components. Does the clutch work properly? | -- | System OK | Go to Step 13
13 | Inspect the clutch assembly for a damaged or worn release bearing. Is the release bearing damaged or worn? | -- | Go to Step 14 | Go to Step 15
14 | Repair or replace the release bearing. Does the clutch work properly? | -- | System OK | Go to Step 15
15 | Check for a faulty clutch disc. Is the clutch disc faulty? | -- | Go to Step 16 | Go to Step 17
16 | Replace the clutch disc. Refer to Clutch Pressure and Driven Plate Replacement . Does the clutch work properly? | -- | System OK | Go to Step 17
17 | Inspect the clutch disc hub at the transmission main drive gear splines. Does the disc assembly hub bind on the transmission main drive gear splines? | -- | Go to Step 18 | --
18 | Replace the clutch disc. Refer to Clutch Pressure and Driven Plate Replacement . Does the clutch work properly? | -- | System OK | --