For 1990-2009 cars

### Diagnostic Aids

If the clutch release bearing is noisy with the clutch fully engaged or during engagement, you will also need to inspect the release bearing for burrs and nicks.

### Test Description

The numbers below refer to the step numbers on the diagnostic table.

1. This step explains there parts and the operation of the clutch system.

2. This step inspects for damage or worn parts.

Step | Action | Yes | No
--- | --- | --- | ---
DEFINITION: The clutch release bearing is noisy with the clutch fully engaged or during engagement.
1 | Did you review the clutch symptom operations and perform the necessary inspections? | Go to Step 2 | Go to Symptoms - Clutch
2 |

1. Remove the transmission. Refer to Transmission Replacement .
2. Inspect the release bearing in the actuator cylinder.

Is the release bearing worn or damaged?

Go to Step 3

Go to Step 4

3 | Replace the release bearing in the clutch actuator. Refer to Clutch Pressure and Driven Plate Replacement . Is the clutch release bearing still noisy? | Go to Step 4 | System OK
4 | Inspect the clutch release bearing or binding on the clutch actuator. Is the release bearing binding? | Go to Step 5 | System OK
5 | Check for weak linkage return spring. Is the return spring weak? | Go to Step 6 | System OK
6 | Replace the return spring. Refer to Clutch Pressure and Driven Plate Replacement . Did you find and repair the condition? | Go to Step 7 | Go to Diagnostic Aids
7 |

1. Install the transmission. Refer to Transmission Replacement .
2. Operate the system in order to verify the repair.

Did you correct the condition?

System OK

Go to Step 1