For 1990-2009 cars

## Rear Compartment Sill Trim Plate Replacement 1st Design

### Removal Procedure

1. Open the rear compartment.
2. Lift up from the inside edge of the sill trim plate in order to release the clips.
3. Remove the rear compartment sill trim plate.

### Installation Procedure

1. Position the rear compartment sill trim plate.
2. Press down in order to engage the retaining clips. Ensure that the retainers lock into place.
3. Close the rear compartment.

## Rear Compartment Sill Trim Plate Replacement 2nd Design

### Removal Procedure

1. Open the rear compartment.
2. Remove the sill trim plate screws.
3. Lift up from the inside edge of the sill plate.
4. Remove the rear compartment sill plate.

### Installation Procedure

1. Position the rear compartment sill plate.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the sill plate screws.

Tighten
Tighten the screws to 1.9 N·m (17 lb in).

3. Close the rear compartment.