For 1990-2009 cars

### Removal Procedure

1. Lower the rear door window.
2. Remove the rear door trim panel. Refer to Rear Side Door Trim Panel Replacement .
3. Remove the rear door water deflector. Refer to Rear Side Door Water Deflector Replacement .
4. Remove the inner sealing strip. Refer to Rear Door Window Belt Inner Sealing Strip Replacement .
5. Remove the outer sealing strip. Refer to Rear Door Window Belt Outer Sealing Strip Replacement .
6. Remove the bolts with secure the regulator to the rear door window.
7. Separate the window from the regulator and lower the window.
8. Remove the lower bolt from the stationary window (2).
9. Remove the stationary window (1) and roll the stationary window forward and remove the stationary window with the run channel weather-strip.

### Installation Procedure

1. Install the stationary window with the run channel weather-strip (1).
2. Install the lower bolt to the stationary window (2).
3. Attach the rear door window to the regulator.
4. Install the bolts which secure the rear door window to the regulator.
5. Install the outer sealing strip. Refer to Rear Door Window Belt Outer Sealing Strip Replacement .
6. Install the inner sealing strip. Refer to Rear Door Window Belt Inner Sealing Strip Replacement .
7. Install the rear door water deflector. Refer to Rear Side Door Water Deflector Replacement .
8. Install the rear door trim panel. Refer to Rear Side Door Trim Panel Replacement .