For 1990-2009 cars

### Removal Procedure

1. Remove the front seat. Refer to Front Seat Replacement - Bucket .
2. Remove the front seat cushion cover. Refer to Front Seat Cushion Cover Replacement .
3. Remove the front seat cushion pad from the front seat cushion frame.

### Installation Procedure

1. Install the front seat cushion pad to the front seat cushion frame.
2. Install the front seat cushion cover. Refer to Front Seat Cushion Cover Replacement .
3. Install the front seat. Refer to Front Seat Replacement - Bucket .