For 1990-2009 cars

## Door Lock Switch Replacement Oldsmobile

### Removal Procedure

1. Use a flat bladed tool in order to pry the lower switch bezel trim panel screw access cover.
2. Remove the lower switch bezel trim panel screws.
3. Use a flat bladed tool in order to pry the lower switch bezel trim panel away from the switch bezel.
4. Use a flat bladed tool in order to pry the front door switch bezel assembly (1) upward. Pry from the rear of the bezel.
5. Disconnect the power door lock switch electrical connectors.
6. Release the power door lock switch retainers.
7. Remove the power door lock switch from the front door switch bezel assembly (1).

### Installation Procedure

1. Install the power door lock switch to the front door switch bezel assembly (1). Ensure that the retainers are locked into position.
2. Connect the power door lock switch electrical connectors.
3. Install the front door switch bezel assembly (1) to the front door trim panel.
4. Install the lower switch bezel trim panel. Ensure that the retainers lock into position.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

5. Install the lower switch bezel trim panel screws.

Tighten
Tighten the lower switch bezel trim panel screws to 10 N·m (89 lb in).

6. Install the lower switch bezel trim panel screw access cover. Ensure the retainers lock into position.

## Door Lock Switch Replacement Pontiac

### Removal Procedure

1. Use a flat-bladed tool in order to pry the front door switch bezel assembly (1) upward. Use inboard pressure against the rear retaining clip.
2. Disconnect the power door lock switch electrical connectors. Slide a flat-bladed tool between the switch and the bezel in order to release the retainers.
3. Remove the power door lock switch from the bezel.

### Installation Procedure

1. Install the power door lock switch to the bezel. Ensure that the retainers are locked into position.
2. Connect the power door lock switch electrical connectors.
3. Install the front door switch bezel assembly (1) to the front door trim panel. Ensure that the retainers are locked into position.