For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Remove the front tire and wheel assemblies. Refer to Tire and Wheel Removal and Installation .
3. Remove the stabilizer shaft. Refer to Stabilizer Shaft Replacement .
4. Remove the stabilizer shaft bushings (1) from the stabilizer shaft (2).

### Installation Procedure

1. Install the stabilizer shaft bushings (1) to the stabilizer shaft (2).
2. Install the stabilizer shaft. Refer to Stabilizer Shaft Replacement .
3. Install the tire and wheel assemblies. Refer to Tire and Wheel Removal and Installation in Tires and Wheels.
4. Lower the vehicle.