For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Loosen the park brake cable at the adjuster.
3. Disconnect the left and right park brake cables from the equalizer (2).
4. Disconnect the intermediate park brake cable from the equalizer (2).
5. Remove the equalizer (2).

### Installation Procedure

1. Connect the left and right park brake cables to the equalizer (2).
2. Connect the intermediate park brake cable to the equalizer (2).
3. Adjust the park brake cable at the adjuster. Refer to Park Brake Adjustment .
4. Lower the vehicle.