For 1990-2009 cars

### Removal Procedure

1. Remove the front seat. Refer to Seat Replacement .
2. Remove the seat back recliner handle. Refer to Seat Back Handle Replacement.
3. Remove the seat cushion outer trim panel. Refer to Seat Cushion Trim Panel Replacement-Outer.
4. Remove the front seat cushion cover J-retainers.
5. Remove the recliner cable retaining screw (4) from the outboard recliner.
6. Disconnect the cable from the outboard recliner mechanism (5). Disconnect the cable from the recliner by rotating the cable downward approximately 90 degrees.
7. Disconnect the cable (2) from the inboard recliner mechanism (1).

Unsnap the cable casing from the inboard recliner.

Disconnect the cable by rotating the cable end downward

8. Remove the cable (2) from the recliner mechanism (1).

### Installation Procedure

1. Connect the new cable (2) to the inboard recliner mechanism (1).
2. Connect the cable (2) onto the outboard recliner mechanism (5).

Important: DO NOT apply excessive force in order to remove the slack. This action may partially unlatch the inboard recliner.

3. Remove the cable slack by pulling rearward on the cable casing.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

4. Install the recliner cable retaining screw (4).

Tighten
Tighten the screw to 4 N·m (35 lb in).

5. Inspect the inboard recliner after installing the cable by pulling back and forth on the recliner seat back arm. Ensure that no play is felt.
6. Inspect the recliner for secure latching.
7. Install the front seat cushion cover J-retainers.
8. Install the seat cushion outer trim panel.

Tighten
Tighten the screws to 1 N·m (9 lb in).

9. Install the seat back recliner handle.

Tighten
Tighten the screws to 1 N·m (9 lb in).

10. Install the front seat. Refer to Seat Replacement .