For 1990-2009 cars

### Removal Procedure

1. Open the left front door.
2. The horn relay is located next to the hood release handle.

Remove the tape securing the horn relay to the body control module electrical harness.

3. Remove the horn relay from the relay socket.

### Installation Procedure

1. Position the horn relay into the relay socket, pressing in until fully seated.
2. Secure the horn relay to the body control module electrical harness with electrical tape.
3. Close the left front door.