For 1990-2009 cars

### Removal Procedure

1. Lower the rear door window.
2. Remove the door panel trim panel. Refer to Rear Side Door Trim Panel Replacement .
3. Pull up on the door inner belt sealing strip (1) in order to release the inner belt sealing strip from the clips.

### Installation Procedure

1. Position the inner sealing strip tabs to the pinchweld (1) on the inner door frame.
2. Install the inner sealing strip, by pressing into place until fully seated.
3. Install the rear door trim. Refer to Rear Side Door Trim Panel Replacement .