For 1990-2009 cars

#### Tool Required

J 36010 Front Cover Crankshaft Seal Installer

### Removal Procedure

1. Remove the engine front cover. Refer to Engine Front Cover Replacement .

Notice: The engine front cover could be damaged if it is not properly supported during seal removal.

2. Support the front cover and drive the oil seal out the timing chain side of the cover.

### Installation Procedure

1. Using J 36010 , position the seal into the front cover by driving the seal from the timing chain side.
2. Install the engine front cover. Refer to Engine Front Cover Replacement .