For 1990-2009 cars

### System Description

The horn system consists of the following components:

• | HORN fuse

• | Horn relay

• | Horn slip ring

• | Horn switch

• | Horn assembly

• | Body control module (BCM)

### System Operation

The vehicle horn system is activated under the following conditions:

• | The horn switch is depressed.

• | The body control module (BCM) commands the horns on. The BCM commands the horns on under any of the following conditions:

- | When the panic button is depressed on the remote control door lock transmitter. For further information, refer to Keyless Entry System Description and Operation in Keyless Entry.

- | When the keyless entry system is used to lock the vehicle, a horn chirp may sound to notify the driver that the vehicle has been locked. The notification feature may be enabled or disabled through personalization. For further information, refer to Keyless Entry System Description and Operation in Keyless Entry.

### Circuit Operation

Battery positive voltage is applied at all times to the horn relay coil and the horn relay switch. Pressing the horn switch applies ground to the horn relay control circuit. The BCM may also apply ground to the horn relay control circuit as described above. When the horn relay control circuit is grounded, the horn relay is energized and battery positive voltage is applied to the horns through the horn control circuit. The horn sounds as long as ground is applied to the horn relay control circuit.