For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
A/C Condenser-to-Radiator Bolts | 10 N·m | 89 lb in
Battery Cable to Battery Bolt | 16 N·m | 12 lb ft
Coolant Inlet Pipe-to-Engine Oil Pan 2.4L | 26 N·m | 18 lb ft
Coolant Inlet Pipe-to-Water Pump Cover 2.4L | 14 N·m | 124 lb in
Coolant Outlet Bolts 2.4L | 26 N·m | 18 lb ft
Coolant Outlet Bolts 3.4L | 25 N·m | 19 lb ft
Fan-to-Shroud Bolts | 5 N·m | 44 lb in
Radiator Lower Support Panel-to-Cradle Bolts | 10 N·m | 89 lb in
Radiator Surge Tank Inlet Pipe Fitting 3.4L | 21 N·m | 15 lb ft
Surge Tank Bolt | 9 N·m | 80 lb in
Surge Tank Cap | 4 N·m | 35 lb in
Transaxle Oil Cooler Fittings at Radiator | 30 N·m | 22 lb ft
Water Pump Cover-to-Block Bolts 2.4L | 26 N·m | 19 lb ft
Water Pump Pulley-to-Pump Bolts 3.4L | 25 N·m | 18 lb ft
Water Pump-to-Water Pump Cover Bolts 2.4L | 14 N·m | 124 lb in
Water Pump-to-Front Cover Bolts 3.4L | 10 N·m | 89 lb in
Water Pump-to-Timing Chain Housing | 26 N·m | 19 lb ft