For 1990-2009 cars

## Electronic Traction Control Switch Replacement Pontiac

### Removal Procedure

1. Remove the Instrument panel (IP) accessory trim plate. Refer to Instrument Panel Accessory Trim Plate Replacement .
2. Remove the IP accessory switch mounting plate bracket screws.
3. Remove the bracket.
4. Depress and release the electronic traction control switch (ETS) retainers. Press the switch out with your thumb. Remove the ETS.

### Installation Procedure

1. Position the ETS to the bracket.
2. Install the switch to the bracket by pressing into place until fully seated.
3. Position the bracket to the accessory trim plate.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

4. Install the IP accessory switch mounting plate bracket screws.

Tighten
Tighten the screws to 3 N·m (27 lb in).

5. Install the instrument panel accessory trim plate. Refer to Instrument Panel Accessory Trim Plate Replacement

## Electronic Traction Control Switch Replacement Oldsmobile

### Removal Procedure

1. Remove the front floor console trim plate. Refer to Front Floor Console Trim Plate Replacement
2. Disengage the traction control switch retainers. Remove the traction control switch.

### Installation Procedure

1. Install the traction control switch to the front floor console trim plate by pressing the switch into place until fully seated.
2. Install the front floor console trim plate. Refer to Front Floor Console Trim Plate Replacement